Genesis Grant

CTEC 402

Homework 3

1. C. B.
2. D.
3. Coaxial cables, these are commonly used among multiple houses in a neighborhood and can be prone to slowing down during peak hours.
4. B.
5. D.
6. B.
7. D.
8. Using the network icon button in the left corner and navigating to the Network and Sharing Center or opening control panel and click Network and Sharing Center
9. Ifconfig
10. Ipconfig
11. Portforwarding and use port 25565
12. D., B., A., C.
13. A., C., D.
14. C.
15. After repairing the cable and you want to ensure everything is working properly, I would suggest pinging again to make sure everything is working and connecting